### No Communication with Left Wagon

Possible Fault Causes:

1. Faulty left Wagon computer power supply
2. Faulty left Wagon computer
3. Faulty wiring
4. Faulty ETSW

Corrective Action

|  |  |  |
| --- | --- | --- |
|  | Yes | No |
| 26BOn the Wagon power distribution panel, verify PC circuit breaker in ON position. Is circuit breaker in ON position? | 3 | 2 |
| 27BSet PC circuit breaker to ON position. Does the problem appear again? | 3 | 7 |
| 28BCheck Ethernet wires are properly connected to PC. Are the wires properly connected? | 5 | 4 |
| 29BConnect Ethernet wires to PC. Does the problem appear again? | 5 | 7 |
| 30BReplace Wagon PC RT (paragraph ‎3.41). Does the problem appear again? | 6 | 7 |
| 31BReplace hub network (paragraph ‎3.19). | - | - |
| 32BPerform Wagon-R and Wagon-L Interactive test (paragraph ‎3.1) | - | - |